Motor Information:

VOUMARD
45000 min-1 (rpm)
360V
2.6kW
6A
750Hz

MR450 No:28316

Mid-1.V/F values set as %50 of Motor V/F values.
06-02=1 (Smart V stall mode) enabled
Startup Freq=0.0
Acc.Ramp=5.0
Dec.Ramp=3.0
5-GRUP Motor parameters:
there is no auto-tuning, 2-pole,
motor rpm set by drive (according to max.freq ve pole number set values).

Rest of them for parameters in factory settings.